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Description
22U network rack enclosures stand out as the preferred choice for floor installations, boasting a robust structure capable of supporting static loads of up to 1700 lbs.
Heavy-duty casters are included to ensure easy and flexible movement. Optional adjustable leveling feet are available to enhance stability and fixation. The quick-open side panels enhance installation and maintenance efficiency, facilitating seamless access to your equipment. 
Choose from multiple sizes to accommodate varying equipment space requirements, with the option for customization to meet specific needs.
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Features
· Both top and bottom cable entries enhance installation flexibility, accommodating various cable configurations.
· Can be shipped disassembled, reducing transportation and storage costs for added efficiency.
· Offers multiple front and rear door styles (optional), providing customization options to suit specific needs.











General Specification
Material                High Quality SPCC 
Material Thickness        Rails 2 mm, Other 1-1.2 mm
Finish                  Power Coating
Color                   RAL7035, Gray
Width                  600 mm
Depth                  600 mm
Height                  22U
Rack Mount              19”
Access                  Front Door/Rear Door/Side Panels
Locking Mechanism        Single Point Locking
Static Loading Capacity     800 kgs/1700 lbs.
Included Accessories       4xCasters, Grounding kits, M6 Screws & Nuts, Keys
Optional Accessories       Fans, Shelves, PDU, Blank Panels


















Ordering Information                                 
	Part No.
	Description

	NSJ6622BP1
	22U Network Rack Cabinet, 600x600mm, Standard Glass Front Door, Solid Metal Rear Door, Gray






 2 / 2
©2025 Ningbo Spring System Integration Co., Ltd., All Rights Reserved. 
Because of the continuous improvements on our products, Ningbo Spring System will reserve the right to change the specifications without prior notice. For more information, please visit us at www.nbspringsys.com.
image1.png
*

PR L XL

S S S S S





image2.png
@




image3.png




